{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":8,"n_cols":8,"rows_kept":8,"merged":[[0,0,0,7],[2,7,6,7],[7,2,7,5]],"flags":["formulas_cached_only"]}
["乐山市妇幼保健院人脸识别系统配置方案清单"]
["序号","设备名称","参数","单位","数量","单价","小计","备注"]
[1,"人脸识别通道","在要求的人行通道安装6路人脸识别终端，要求实现人脸录像、抓拍、报警、上传等功能","路",6,null,null,"医院现有监控报警平台品牌为：大华"]
[2,"人脸后台处理终端","能对通道抓拍的人脸进行处理，如有黑名单人员出现能立即录像、存储及报警和上传。","套",1]
[3,"配套线管材","含完成系统安装及调试所需的所有线材、管件及辅助材料等。","项",1]
[4,"系统对接与接入","★要求本子系统能与医院原有安防综合管理平台无缝对接，院方可通过医院原有安防综合管理平台对本子系统进行日常操作及管理，实现人脸识别、人脸抓拍、报警、信息统计及查询等功能（须针对此项功能提供相关承诺函原件）。","项",1]
[5,"安装调试"]
[6,"合计","含税"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}